Program.cs :-

* Inside program.cs file Main method are available.
* Means start Running program from here

Inside main method create one networkInterface[] array

* Provides configuration and statistical information for a network interface.
* This class encapsulates data for network interfaces, also known as adapters, on the local computer. You do not create instances of this class; the [GetAllNetworkInterfaces](https://docs.microsoft.com/en-us/dotnet/api/system.net.networkinformation.networkinterface.getallnetworkinterfaces?view=net-6.0) method returns an array that contains one instance of this class for each network interface on the local computer.

Then create two variable one is string and second is Boolean.

* String sMacAddress = string.Empty; //set string as empty
* bool isGeniuene = false; // isGeniuene value is false

IPInterfaceProperties:-

* C# IPInterfaceProperties type Provides information about network interfaces that support Internet Protocol version 4 (IPv4) or Internet Protocol version 6 (IPv6).

sMacAddress = adapter.GetPhysicalAddress().ToString();

* Get mac address and store inside sMacAddress.
* Mac address store in string format.

After that check mac address is match or not using if.

* mac address is match then set isGeniuene value true.

After that check

* if(isGeniuene)//condition is true then go inside this if block {}

else

{

MessageBox.Show("Please insert License file to proceed...!");  
}

inside if create one local variable bool mutexCreated = true;

Mutex

* A Mutex is a synchronization primitive that can also be used for interprocess synchronization. When two or more threads need to access a shared resource at the same time, the system needs a synchronization mechanism to ensure that only one thread at a time uses the resource. Mutex is a synchronization primitive that grants exclusive access to the shared resource to only one thread. If a thread acquires a Mutex, the second thread that wants to acquire that Mutex is suspended until the first thread releases the Mutex.
* In short, A mutual exclusion ("Mutex") is a mechanism that acts as a flag to prevent two threads from performing one or more actions simultaneously. The entire action that you want to run exclusively is called a critical section or protected section.
* A critical section is a piece of code that accesses a shared resource (data structure or device) but the condition is that only one thread can enter in this section at a time.

After that check condition

if(mutexCreated) //true

{

Application.Run(new MasterForm()); //call MasterForm()

}

**MasterFrom.cs :-**

* Inside MasterFrom.cs file all aubut the masterfrom backend codding work.

**InitializeComponent();**

* This method call the designer class
* Example:

**MasterFrom.Designer.cs**

After that call **CheckHalconLicense();** method and check condition

If condition is true then return true otherwise return false.

And return value store inside HalconLicense Boolean variable.

* if (HalconLicense) //true
* Inside if

hSmartWindowControl1.HKeepAspectRatio = true;

hSmartWindowControl2.HKeepAspectRatio = true;

win\_result1 = hSmartWindowControl1.HalconWindow;

win\_result2 = hSmartWindowControl2.HalconWindow;

// hSmartWindowControl1.SetFullImagePart(null);

// hSmartWindowControl2.SetFullImagePart(null);

Cam1ResultDict = new ConcurrentDictionary<int, bool>();

Cam2ResultDict = new ConcurrentDictionary<int, bool>();

FinalResultDict = new ConcurrentDictionary<int, bool>();

ReadCalibration\_files();

* **After that check camera used using if else statement.**

if (usedcamera == "IDS")

{

Cam2 = initCamera(Cam2, 1); // call initCamera() method.

if (Cam2 != null) //check condition

{

Cam2.EventFrame += new System.EventHandler(this.onFrameEvent\_cam2);

// call onFrameEvent\_cam2() method

}

}

else if (usedcamera == "FLIR")

{

InitImageEventListener(); //call this method

}

else if (usedcamera == "HIKVISION")

{

initcommunication(); //call initcommunication() method

DeviceListAcq(); // call DeviceListAcq()

Init(); // call Init() method

}